**Project # 1: Spatial and Frequency Filtering**  
*CSC 391: Computer Vision*  
Caroline Li  
February 6, 2019

**3.2.1 Smoothing and denoising**

Below are the result of using the Gaussian and median filters of different sizes on the noisiest puppy image. As we can see, the larger the filter the smoother the image becomes so the less information we have about the subject for both filters. Comparing the 27 x 27 Gaussian filter with the 27 x 27 median filter, the Gaussian filter appears to make the whole image look equally blurry while the median filter appears smooth in areas of similar colors and intensities, and maintains sharp edges in areas such as where the white blanket touches the dark background, or where the puppy’s dark ear is next to its white fur. So the median filter appears to maintain sharp edges where there’s a clear distinction between different values, but only if these are large areas; if we look at where the puppy’s eyes are, it’s hard to see where exactly they are, which may be a result of the size of the filter.


|  |  |
| --- | --- |
| **Gaussian Filter** | **Median Filter** |
| 3 x 3 | 3 x 3 |
| 9 x 9 | 9 x 9 |
| 27 x 27 | 27 x 27 |


If we look at how running these filters on less noisy images and compare, we can see that the results from the Gaussian filter are pretty similar, whereas with the median filter on the less noisy image, we can see even more edges such as the top of the puppy’s head and in the puppy’s shadow, and edges that we see in the noisier image are even more sharp in the less noisy image.

|  |  |
| --- | --- |
| **27 x 27 Gaussian Filter** | **27 x 27 Median Filter** |
| 0.02 Noisy Image | 0.02 Noisy Image |
| 0.50 Noise Image | 0.50 Noisy Image |




**3.2.2 Edge detection**

Using the Canny edge detector with the non-noisy image, we can see outlines of the puppy’s ear, nose, coat, and the blanket. With the noisy image, however, edge detection appears to be random noise.





With the field images, while vegetation appears quite noisy, it is easy to distinguish where there is a body of water or a road.



**4.2 Frequency Analysis**

Below is a comparison of the Fourier coefficients for the original and noisy image of the puppy. We can see that these images are fairly similar, though the noisy image has more values further away from zero which is likely because of the added noise. The difference doesn’t appear that great in these plots aside from some of the values being further away from the center in the noisy image.

|  |  |
| --- | --- |
|  |  |
| Original Image | Noisy Image |

Below are comparisons using the field images. We see that for the first two images, the Fourier coefficients show higher values around 0, probably because of the contrast between the foliage and sand, as well as the foliage and the dark body of water, in comparison to just foliage in the last picture shown.

|  |  |
| --- | --- |
| **Image** | **Fourier Coefficients** |
| window-00-02 |  |
| window-00-04 |  |
| window-00-06 |  |

When comparing the log plots of the magnitude of the Fourier coefficients between the original and noisy images of the puppy, we can see that the noisier the image is, the higher the values are away from the image. This is because of the added noise in the image, which disperses light and dark values all over the image, thus altering the magnitudes that we see.

|  |  |
| --- | --- |
|  |  |
| Original Image | Noisy Image |

The following images show the original puppy image when lower frequencies are zeroed out and when higher frequencies are zeroed out.

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Original Grayscale Image | Zero Low Frequencies | Zero High Frequencies |

\_ What is the e\_ect of removing (zero-ing out) Fourier coe\_cients on the image reconstructed using

the inverse 2-D DFT? Observe what happens when Fourier coe\_cients in the center of the magnitude

plot around F(0; 0) (i.e. the low frequencies) are zero-ed out and compare to what happens when the

Fourier coe\_cients away from the center (i.e. high frequencies) are zero-ed out. Observe what you get

and draw conclusions as to how this might be useful for smoothing or edge detection